**Solar Panel Emblem Requirements**





**N.J.A.C. 5:70-2.21**

**(a) Emblems shall be permanently affixed to the front of the structure**

 **1. Shall be a Maltese cross shape, constructed of durable material, with white reflective background with red letters**

 **i. Minimum 6-inch x 6-inch in size**

**iii. Center of the Maltese cross must be a circle or oval 3 inch in diameter**

**v. PV shall be located in the middle of the circle of the Maltese. The wording ROOF MOUNTED and/or ADJACENT shall be located immediately beneath the Maltese to identify location of solar panels.**